

**New Codie II (China)**

One-Piece Toilet

CP-2033 (305mm RI)

CP-2034 (400mm RI)

**FEATURES**

* **Types of Flushing**: Washdown
* **Design**: Modern design with wider size for more comfortable seating
* **Trapway**: Concealed trapway
* **Seat**: Comfort Seat and Slow Close
* **Water Saving**: 3/4.5L water saving

**STANDARDS CRITERIA**

* TIS-792:2001
* GB 6952-2005
* PNS 156:2010
* MS 1522:2007
* SS 378-1996
* ASME-A112.19.2-2008

****

**SPECIFICATIONS**

* **Litres Per Flush**: 3/4.5 lpf
* **P/S-Trap/Bowl Shape**: S trap, elongated
* **Roughing in:** 305mm, 400mm floor discharge
* **Overall Dimensions (LxBxH)**:

L709xW350xH712mm

* **Height to Rim**: 400mm
* **Material**: Vitreous China

**DIMENSIONAL DRAWING**





**COLOR AVAILABILITY**

* White only(0)

 **INCLUDED COMPONENTS**

* PP Slow Closing Seat CCASC033-0200430C0
* Angle Valve and Water Supply Hose CC1-CN511MSA009182

**STANDARDS CRITERIA**

* China GB 6952-2005

This document is the property of American Standard. It can neither be reproduced, nor communicated, without authorization.

American Standard reserves the right to change dimensions and specifications without notice; we assume no liability for the use of obsolete dimensions.

**STANDARDS CRITERIA**

* TIS-792:2001
* GB 6952-2005
* PNS 156:2010
* MS 1522:2007
* SS 378-1996
* ASME-A112.19.2-2008