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Single Hole Basin Mixer
FFAS1701-101500ZN0
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FEATURES
· Low lead brass, strong and durable
· Grohe High quality ceramic valve for longer usage
· Ceramic cartridge tested = 500,000 times
· Neoperl aerator PCA 1.5 GPM 
· Without pop-up drain
· With normal packaging
· Flow rate @ WELS 5 Stars
· WMK certificated

SPECIFICATIONS
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Basin mixer faucet
1-hole installation: lever handle (cold & hot)

Spout reach: 100.8 mm

Spout height:  98.5 mm


FINISHES AVAILABILITY
Chrome (- CP)
AWARDS WON
·  N/A

SHIPPING WEIGHT
Product gross weight:  1.58kg /set 
Product net weight:  1.37kg /set 
STANDARDS CRITERIA
 AS/NZS 3718   
 AS/NZS 6400 
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