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AccuStream Extended Vessel Sensor Faucet
1130400000
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FEATURES
· A grade brass body, strong and durable;
· DC 6V (CRP2 Lithium Battery) or AC220V ;
· Automatic adjustment of sensing distance;
· Sensor technological innovation , no error operation when the sensor face to the mirror;
· Flow rate ≤ 4.5L/Min at  1bar

SPECIFICATIONS
Sensor installed at the spout
Faucet Reach: 145.7mm

Faucet  Height:  256.4mm

FINISHES AVAILABILITY
Chrome (- CP)
AWARDS WON
·  N/A


SHIPPING WEIGHT
Product net  weight:  1.85kg/set 
Product gross  weight:  2.1 kg/set 
STANDARDS CRITERIA
QB1334
This document is the property of American Standard. It can neither be reproduced, nor communicated, without authorization.
American Standard reserves the right to change dimensions and specifications without notice, we assume no liability for the use of obsolete dimensions.
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