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Square Wall Outlet With Holder
FFAS9143-000A00BT0
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FEATURES
· Brass body, PVD plated 
· Brass escutcheon, PVD plated 
· With normal packaging
· Flow rate @ 0.1MPa:  19.6  L/min 
SPECIFICATIONS

R 1/2” for inlet 
G 1/2” for outlet



FINISHES AVAILABILITY
PVD Polished Hard Grophite
AWARDS WON
 N/A
SHIPPING WEIGHT 
Product net weight: 0.61 kg 
Product gross weight: 0.71 kg
STANDARDS CRITERIA
 GB 18145-2014 

This document is the property of American Standard. It can neither be reproduced, nor communicated, without authorization.
American Standard reserves the right to change dimensions and specifications without notice, we assume no liability for the use of obsolete dimensions.
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