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Milano
Exposed Bath & Shower Mixer
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FFAS0911-601500BF0


FEATURES
· A grade brass, strong and durable
· High quality ceramic valve for longer usage
· Ceramic cartridge tested = 500,000 times
· Neoperl aerator 
· 5-Functions hand shower
· With shower hose & hanger
· With normal packaging
· Flow rate @ 0.1MPa: 10.5 L/min for spout
· Flow rate @ 0.1MPa: 6.5 L/min for shower
SPECIFICATIONS
Exposed Bath & Shower Mixer Faucet
2-Hole Installation: lever handle (cold & hot)

Spout Reach: 170 mm


FINISHES AVAILABILITY
Chrome (- CP)
AWARDS WON
·  N/A

SHIPPING WEIGHT
Product gross weight:  3.1kg/set 
Product net weight:  2.8kg/set 
STANDARDS CRITERIA
GB 18145-2014 

This document is the property of American Standard. It can neither be reproduced, nor communicated, without authorization.
American Standard reserves the right to change dimensions and specifications without notice, we assume no liability for the use of obsolete dimensions.
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