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[image: ][image: ]250mm R ou nd Air-in Brass Rain Shower Head 
STANDARD SPECIFICATION

· Brass body
· Brass front panel, Chromium plating for durable finish 
· Brass back cover, Chromium plating for durable finish
· Brass connector, Chromium plating for durable finish
· Silicon nipple
· Flow rate @ 0.1 MPa (with regulator) 5.37 L/min 


PRODUCT WEIGHT: 1.32 Kg

APPLICABLE CODES & STANDARDS:
 
· GB 23447-2009
STANDARDS CRITERIA
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