

Milano



Exposed Bath & Shower Mixer

FFAS0911-629500BC0

FFAS0911-602501BF0

FFAS0911-6T2501BT0



**FEATURES**

* A grade brass, strong and durable
* High quality ceramic valve for longer usage
* Ceramic cartridge tested = 500,000 times
* Neoperl aerator
* Without shower kits
* With normal packaging
* Flow rate @ 0.1MPa: 7.78 L/min for spout
* Flow rate @ 0.1MPa: 10.3 L/min for shower

**SPECIFICATIONS**

Exposed Bath & Shower Mixer Faucet

2-Hole Installation: lever handle (cold & hot)

Spout Reach: 127 mm

**FINISHES AVAILABILITY**


Chrome (- CP)

**AWARDS WON**

* N/A

**DIMENSIONAL DRAWING**


**SHIPPING WEIGHT**

Product weight: 2.31 kg

**STANDARDS CRITERIA**

TIS 2066-2552

GB 18145-2014



This document is the property of American Standard. It can neither be reproduced, nor communicated, without authorization.

American Standard reserves the right to change dimensions and specifications without notice, we assume no liability for the use of obsolete dimensions.