

**Milano**

Single Hole Vessel Faucet

FFAS0902-102501BF0



**FEATURES**

* A grade brass, strong and durable
* Germanic ceramic valve for longer usage
* Ceramic cartridge tested = 500,000 times
* Neoperl aerator
* Without pop-up drain
* With normal packaging
* Flow rate @ 0.42MPa: 5.5 L/min for spout

 **SPECIFICATIONS**

Basin mixer faucet

1-hole installation: lever handle (cold & hot)

Spout reach: 153 mm

Spout height: 238mm

**FINISHES AVAILABILITY**

**DIMENSIONAL DRAWING**

Chrome (- CP)

**AWARDS WON**

* N/A

**SHIPPING WEIGHT**

Product gross weight:2.55kg/set

Product net weight: 2.05kg/set

**STANDARDS CRITERIA**

GB 18145-2014



This document is the property of American Standard. It can neither be reproduced, nor communicated, without authorization.

American Standard reserves the right to change dimensions and specifications without notice, we assume no liability for the use of obsolete dimensions.