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Kitchen Mixer
Agate Dual Spray Pull-out Kitchen Faucet_243_APAC
1009262430
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FEATURES
· Metal body, strong and durable
· High quality 28# ceramic disc cartridge (Germany)  for longer usage
· Ceramic cartridge tested = 500,000 times
· Two-function spray 
· Pull-down spray
· With normal packaging
· Flow rate @ 1bar:  3.1 L/min for spout
SPECIFICATIONS
G1/2” 600mm flexible hose 
1- Hole Installation: lever handle (cold & hot)
Spout Reach: 226 mm Spout Height 210mm


FINISHES AVAILABILITY
MB 243
AWARDS WON
·  N/A


SHIPPING WEIGHT
Product gross weight:  3.0 kg 
Product net weight:      2.8  kg

STANDARDS CRITERIA
GB 18145-2014
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American Standard reserves the right to change dimensions and specifications without notice, we assume no liability for the use of obsolete dimensions.
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