

**Acacia E**



vdalve & flexible hose CCAS2074-2200400C0

**FEATURES**

* Use thick acrylic sheets, has better [heat](http://dict.youdao.com/w/heat/#keyfrom=E2Ctranslation) [retaining](http://dict.youdao.com/w/retaining/#keyfrom=E2Ctranslation) [property](http://dict.youdao.com/w/property/#keyfrom=E2Ctranslation) and more durable
* White super thin large flat water combine with the bath tub is fashion and generous
* Advanced seamless splicing technology makes skirt and cylinder splicing seamless, which show strong sense of design and easy to clean and maintain
* Wide cylinder design on one side as a practical storage area bring better practicability.



CT-6719.056.04\Acacia E 1.7M Acrylic Seamless Floor-standing Tub

BTAS6719-032AS00C5

**SPECIFICATIONS**

* Installation Type: Free Standing
* Dimension: 1700x 850 x 580 mm
* Includes overflow hole
* Material: Acrylic

**COLOR AVAILABILITY**

* White only(0)

**INCLUDED COMPONENTS**

* Bath drain


**SHIPPING WEIGHT**

* Net Weight: 47 Kg
* Gross Weight: 56 Kg

**STANDARD CRITERIA**

* JC/T 779-2010

**DIMENSIONAL DRAWING**



This document is the property of American Standard. It can neither be reproduced, nor communicated, without authorization.

American Standard reserves the right to change dimensions and specifications without notice; we assume no liability for the use of obsolete dimensions.