

Kastello



One Piece Toilet

CCAS2025/2026

 **FEATURES**

* SiphonMax with Power Rim
* Water Saving
* ArmorLid with Slow Closing
* Aqua Ceramic, Comfort Clean Glaze

**SPECIFICATIONS**

Flushing Type: 3.8 Litres per flush

Flushing Activation: Side Lever

Roughing in : S-trap 305/400mm

Bowl shape: Elongate

Overall Dimensions: L743xW381xH695mm


Height to rim: 390 mm

Material: Vitreous China

**SHIPPING WEIGHT**

**DIMENSIONAL DRAWING**

Net Weight: 51 KG


Gross Weight: TBD

**INCLUDED COMPONENTS**

Quick installation tape

Installation manual

**STANDARDS CRITERIA**

* GB6952-2015
* KIS-2012

This document is the property of American Standard. It can neither be reproduced, nor communicated, without authorization.

American Standard reserves the right to change dimensions and specifications without notice; we assume no liability for the use of obsolete dimensions.