



FFAS1M01-101500BF0

Single-Hole Basin Mixer Faucet



**FEATURES**

* Modern design that can fit with any style of bathroom
* **Cold-Start handle** for saving energy
* Ceramic disc valve for a life time use
* Strong brass construction
* Nickel and chromium plating for durable finish
* M24x1 1.5GPM PCA Aerator
* With Pop-up drain
* Flow Rate @ 0.1 MPa : 3.5 L/Min

**SPECIFICATIONS**

Basin mixer faucet

1-hole installation: lever handle (cold & hot)

Spout reach: 107 mm

Spout height: 90 mm

**DIMENSIONAL DRAWING**



**FINISHES AVAILABILITY**

Chrome (- CP)

**AWARDS WON**

* N/A

**SHIPPING WEIGHT**

Product gross weight: 1.45kg /set

Product net weight: 1.25kg /set

**STANDARDS CRITERIA**

TIS 2067-2552

GB 18145-2014



This document is the property of American Standard. It can neither be reproduced, nor communicated, without authorization.

American Standard reserves the right to change dimensions and specifications without notice, we assume no liability for the use of obsolete dimensions.