

**Shower Head**



FFASTS01-006500BF0

10" Round Stainless Steel Rain Shower Head with Air-in (w/o shower arm)



**STANDARD SPECIFICATION**

* SUS304 SS body, mirror polishing
* Brass connector, chromium plating for durable finish
* Gray silicone nozzle
* Air -In Technology
* W/o shower arm
* W/ DIY white box
* Flow rate @ 0.1 MPa (with regulator) 4.5 L/min

**PRODUCT WEIGHT:** 1.2 Kg

**APPLICABLE CODES & STANDARDS:**

* TIS 2066-2552

**STANDARDS CRITERIA**

