

**Shower Head**



FFASTS06-006500BF0

Square 300x300 mm Brass Rain Shower Head with Air-in (w/o shower arm)

**STANDARD SPECIFICATION**

* Brass front body, chromium plating for durable finish
* Stainless steel back body, chromium plating for durable finish
* Brass connector, chromium plating for durable finish
* Gray silicon nozzle
* Air -In Technology
* W/o shower arm
* W/ DIY white box
* Flow rate @ 0.1 MPa (with regulator) 6.1 L/min

**PRODUCT WEIGHT:** 2.5 Kg

**APPLICABLE CODES & STANDARDS:**

* TIS 2066-2552

**STANDARDS CRITERIA**



